**CH340 driver installation instructions**

For applications that use the USB interface, you need to install the CH340 driver (USB serial port driver). You can get the driver from the manufacturer of the monitor.


1. Unzip“stc-isp-15xx-v6.86h.zip”file.
2. In the unzip file, find the "USB to UART Driver" folder, double click Open.
3. Double click to run the "ch341ser.exe" file in the open file.



4、Click the arrow pointing to "Install", enter the next step.



5、The following interface will appear, and then click "OK", and the drive installation is done.



6、After successful installation of the driver in Windows 8.1 or earlier versions, put the customer display USB cable to Insert into the computer, when you browse a computer hardware device, it will be displayed in the computer as follows:

The port number of the arrow is the communication port number of the display and other software.

